# temperature_sht

SHTxx, for Sensirion humidity and temperature sensors

Author | Eur van Andel, eur@fiwihex.nl Copyright © 2008
Adapted-by |
Compiler | =2.4h

Description

    The Sensirion SHT1x/SHT7x is a single chip relative humidity and
    temperature multi sensor module comprising a calibrated digital output.
    It comes in 5 flavors, with different accuracy and package style:
    sensor   hum acc  temp acc    package
    SHT10    4.5%     0.5C        SMD (LCC)
    SHT11    3.0%     0.4C        SMD (LCC)
    SHT15    2.0%     0.3C        SMD (LCC)
    SHT71    3.0%     0.4C        4-pin single-in-line
    SHT75    1.8%     0.3C        4-pin single-in-line
    all consist of the same silicon: the less accurate models are sold cheaper.
    My experience is mixed: I've seen some consistent +2C offset in temperature,
    but good humidty measurements. The 4-pin package breaks when you touch it.
    The SMD package has naked tracks underneath: you can't route under it!
    If exposed to >95% RH for 10 minutes, these sensors will go beserk and need
    <60% RH for an hour to recover. You might try heating them.
    protocol is close to I2C, but not the same. Remember to pull up DATA.
    0b0000_0011  starts temperature measurement
    0b0000_0101  starts humidity measurement
    device returns three bytes: MSB, LSB and CRC
    this library doesn't perform any CRC check

Sources

    http://www.sensirion.com/en/01_humidity_sensors/00_humidity_sensors.htm

Dependencies

- delay

## Summary

### Global variables/contants

### Procedures

- `read_raw_hum_sht(byte out MSB, byte out LSB, byte out CRC)`
- `read_hum_word_sht(word out hum)`
- `sht_get_data(byte out x)`
- `sht_start()`
- `sht_put_ack()`
- `sht_wait_ack_out(bit out ack)`
- `sht_conn_reset()`
- `sht_wait_ack()`
- `sht_reset()`
- `read_centicelsius_temp_sht(sword out centicelsius)`
- `sht_put_data(byte in x)`
- `read_celsius_temp_sht(sbyte out celsius)`
- `read_hum_sht(byte out hum)`
- `read_raw_temp_sht(byte out MSB, byte out LSB, byte out CRC)`

### Functions

## API details

### Global variables/contants

### Procedures

- `read_raw_hum_sht(byte out MSB, byte out LSB, byte out CRC)`

      read raw 12-bit humidity from SHT
      default value of resolution bit is 12 bit RH
      SHT takes 55 ms for measurement @ 12 bits
      we will wait 70 ms
      SHT may only be switched on for 10% of the time because of self-heating
      so this measurement can only happen every 500ms

- `read_hum_word_sht(word out hum)`

      read humidity from SHT, result in word precision 0.01%RH
      SHT may only be switched on for 10% of the time because of self-heating
      so this measurement can only happen every 500ms

- `sht_get_data(byte out x)`

      receive one byte from the SHT

- `sht_start()`

      send start
      _____         ________
      DATA:      |_______|
      ___     ___
      SCK : ___|   |___|   |______

- `sht_put_ack()`

      send ACK

- `sht_wait_ack_out(bit out ack)`

  No documentation found

- `sht_conn_reset()`

      reset SHT interface, must be followed with sht_start and command

- `sht_wait_ack()`

      wait for ACK, but continue after 1 ms

- `sht_reset()`

      reset SHT

- `read_centicelsius_temp_sht(sword out centicelsius)`

      read Celcius temperature from SHT
      with 0.01 C resolution, result is sword type, so -327.68 .. +327.68 C
      SHT takes 320 ms for measurement @ 14 bits
      we will wait 400 ms
      SHT may only be switched on for 10% of the time because of self-heating
      so this measurement can only happen every four seconds!

- `sht_put_data(byte in x)`

      send one byte to the SHT

- `read_celsius_temp_sht(sbyte out celsius)`

      read Celcius temperature from SHT
      with 1 C resolution, result is sbyte type, so -126...+127C
      SHT takes 320 ms for measurement @ 14 bits
      we will wait 400 ms
      SHT may only be switched on for 10% of the time because of self-heating
      so this measurement can only happen every four seconds!

- `read_hum_sht(byte out hum)`

      read humidity from SHT, result in byte precision 1%RH
      SHT may only be switched on for 10% of the time because of self-heating
      so this measurement can only happen every 500ms

- `read_raw_temp_sht(byte out MSB, byte out LSB, byte out CRC)`

      read raw 14-bit temperature from SHT
      default value of resolution bit is 14 bit temperature
      SHT takes 320 ms for measurement @ 14 bits
      we will wait 330 ms
      SHT may only be switched on for 10% of the time because of self-heating
      so this measurement can only happen every two seconds!

### Functions

## Related samples

No sample found