# i2c_software

i2c_software

Author | Wouter van Ooijen, Copyright © 1998, 1999 Wouter van Ooijen
Adapted-by | Joep Suijs.
Compiler | >=2.4g

Description

    Software implementation of I2C (single) master.

     Define i2c pins like:
    alias i2c_scl            is pin_c3
    alias i2c_scl_direction  is pin_c3_direction
    alias i2c_sda            is pin_c4
    alias i2c_sda_direction  is pin_c4_direction

    const word _i2c_bus_speed = 1 ; * 100kHz

Dependencies

- delay

## Summary

### Global variables/contants

### Procedures

- `i2c_initialize()`
- `i2c_stop()`
- `i2c_start()`
- `i2c_restart()`

Private

- `_i2c_bit_out(bit in x)`
- `_i2c_bit_in(bit out x)`
- `_i2c_wait()`

### Functions

- `i2c_transmit_byte( byte in x ) return bit`
- `i2c_receive_byte(bit in ack) return byte`

## API details

### Global variables/contants

### Procedures

- `i2c_initialize()`

      i2c_initialize - initialize the software i2c bus

      The output latch values are always low,
      the lines are switched open-collector fashion by
      manipulating the direction registers.

- `i2c_stop()`

      i2c_stop - output a stop condition

- `i2c_start()`

      i2c_start - output a start condition

- `i2c_restart()`

      i2c_restart - output a (re)start condition

      A restart is a start without a previous stop.
      This procedure is provided as part of the API to maintain compatibility
      with the i2c hardware master lib.

Private

- `_i2c_bit_out(bit in x)`

      _i2c_bit_out- output a single bit (for internal use only)

- `_i2c_bit_in(bit out x)`

      _i2c_bit_in- input a single bit (for internal use only)

- `_i2c_wait()`

      _i2c_wait - wait for a change to settle (for internal use only)

      The delay is determined by i2c_bus_speed and is 1/4 of the cycle time.
      Given the delay resolution of 1 us and all actions required by
      i2c_software routines, the actual bus speed will be lower then the
      configured maximum.

### Functions

- `i2c_transmit_byte( byte in x ) return bit`

      i2c_transmit_byte - output one byte

      return true = okay, false = no ack received

- `i2c_receive_byte(bit in ack) return byte`

      i2c_receive_byte - read one byte

      The ACK flag indicated if the byte read must be acked.
      In general, all bytes read by the master are acked, except the last one.
      Failing to NACK the last byte read will give unpredictable results.
      (Often it will provide repeatable sequences, where one out of 2 to 4 of
      the reads from a specific device is correct. You are warned!)

## Related samples

Here are the list of samples which use this library:

16f648a | 16f648a_lcd_hd44780_pcf8574.jal
16f648a | 16f648a_i2c_sw_master_echo.jal
16f648a | 16f648a_i2c_sw_l1.jal
16f648a | 16f648a_i2c_sw_l0.jal
16f648a | 16f648a_i2c_sw_master_check_bus.jal
16f648a | 16f648a_lcd_dsm0822a.jal
16f723 | 16f723_lcd_dsm0822a.jal
16f723 | 16f723_i2c_sw_master_echo.jal
16f723 | 16f723_i2c_sw_l0.jal
16f723 | 16f723_lcd_hd44780_pcf8574.jal
16f723 | 16f723_i2c_sw_master_check_bus.jal
16f723 | 16f723_i2c_sw_l1.jal
16f73 | 16f73_i2c_sw_master_echo.jal
16f73 | 16f73_i2c_sw_master_check_bus.jal
16f73 | 16f73_lcd_hd44780_pcf8574.jal
16f73 | 16f73_lcd_dsm0822a.jal
16f73 | 16f73_i2c_sw_l0.jal
16f73 | 16f73_i2c_sw_l1.jal
16f877 | 16f877_i2c_sw_l1.jal
16f877 | 16f877_lcd_dsm0822a.jal
16f877 | 16f877_lcd_hd44780_pcf8574.jal
16f877 | 16f877_24lc256.jal
16f877 | 16f877_i2c_sw_master_echo.jal
16f877 | 16f877_i2c_sw_l0.jal
16f877 | 16f877_i2c_sw_master_check_bus.jal
16f877a | 16f877a_ds1307_sw.jal
16f877a | 16f877a_24lc256.jal
16f877a | 16f877a_lcd_dsm0822a.jal
16f877a | 16f877a_i2c_sw_master_check_bus.jal
16f877a | 16f877a_lcd_hd44780_pcf8574.jal
16f877a | 16f877a_i2c_sw_l1.jal
16f877a | 16f877a_i2c_sw_l0.jal
16f877a | 16f877a_servo_rc_master_dedicated_master_i2c.jal
16f877a | 16f877a_i2c_sw_master_echo.jal
16f88 | 16f88_i2c_sw_master_check_bus.jal
16f88 | 16f88_i2c_sw_l0.jal
16f88 | 16f88_lcd_hd44780_pcf8574.jal
16f88 | 16f88_lcd_dsm0822a.jal
16f88 | 16f88_i2c_sw_master_echo.jal
16f88 | 16f88_i2c_sw_l1.jal
18f14k50 | 18f14k50_i2c_sw_master_check_bus.jal
18f14k50 | 18f14k50_i2c_sw_master_echo.jal
18f14k50 | 18f14k50_i2c_sw_l1.jal
18f14k50 | 18f14k50_lcd_hd44780_pcf8574.jal
18f14k50 | 18f14k50_i2c_sw_l0.jal
18f14k50 | 18f14k50_lcd_dsm0822a.jal
18f2450 | 18f2450_i2c_sw_l0.jal
18f2450 | 18f2450_lcd_hd44780_pcf8574.jal
18f2450 | 18f2450_i2c_sw_master_echo.jal
18f2450 | 18f2450_i2c_sw_l1.jal
18f2450 | 18f2450_i2c_sw_master_check_bus.jal
18f2450 | 18f2450_lcd_dsm0822a.jal
18f2520 | 18f2520_lcd_hd44780_pcf8574.jal
18f2520 | 18f2520_i2c_sw_l0.jal
18f2520 | 18f2520_i2c_sw_l1.jal
18f2520 | 18f2520_lcd_dsm0822a.jal
18f2520 | 18f2520_i2c_sw_master_check_bus.jal
18f2520 | 18f2520_i2c_sw_master_echo.jal
18f2550 | 18f2550_lcd_dsm0822a.jal
18f2550 | 18f2550_i2c_sw_master_check_bus.jal
18f2550 | 18f2550_i2c_sw_l0.jal
18f2550 | 18f2550_i2c_sw_l1.jal
18f2550 | 18f2550_lcd_hd44780_pcf8574.jal
18f2550 | 18f2550_i2c_sw_master_echo.jal
18f2620 | 18f2620_i2c_sw_master_check_bus.jal
18f2620 | 18f2620_lcd_hd44780_pcf8574.jal
18f2620 | 18f2620_i2c_sw_master_echo.jal
18f2620 | 18f2620_i2c_sw_l1.jal
18f2620 | 18f2620_i2c_sw_l0.jal
18f2620 | 18f2620_lcd_dsm0822a.jal
18f452 | 18f452_i2c_sw_master_echo.jal
18f452 | 18f452_24lc256.jal
18f452 | 18f452_pressure.jal
18f452 | 18f452_i2c_sw_master_check_bus.jal
18f452 | 18f452_i2c_sw_l1.jal
18f452 | 18f452_lcd_hd44780_pcf8574.jal
18f452 | 18f452_servo_rc_master_dedicated_master_i2c.jal
18f452 | 18f452_i2c_sw_l0.jal
18f452 | 18f452_lcd_dsm0822a.jal
18f4525 | 18f4525_24lc256.jal
18f4550 | 18f4550_lcd_hd44780_pcf8574.jal
18f4550 | 18f4550_lcd_dsm0822a.jal
18f4550 | 18f4550_i2c_sw_l0.jal
18f4550 | 18f4550_i2c_sw_l1.jal
18f4550 | 18f4550_i2c_sw_master_echo.jal
18f4550 | 18f4550_i2c_sw_master_check_bus.jal
18f4550 | 18f4550_24lc256.jal
18f4620 | 18f4620_servo_rc_master_dedicated_master_i2c.jal
18f4620 | 18f4620_i2c_sw_l1.jal
18f4620 | 18f4620_i2c_sw_l0.jal
18f4620 | 18f4620_lcd_hd44780_pcf8574.jal
18f4620 | 18f4620_lcd_dsm0822a.jal
18f4620 | 18f4620_24lc256.jal
18f4620 | 18f4620_i2c_sw_master_check_bus.jal
18f4620 | 18f4620_i2c_sw_master_echo.jal
18f67j50 | 18f67j50_lcd_dsm0822a.jal
18f67j50 | 18f67j50_i2c_sw_l0.jal
18f67j50 | 18f67j50_i2c_sw_l1.jal
18f67j50 | 18f67j50_lcd_hd44780_pcf8574.jal
18f67j50 | 18f67j50_i2c_sw_master_check_bus.jal
18f67j50 | 18f67j50_i2c_sw_master_echo.jal