# pps

Peripheral Pin Select (PPS) library

Author | Sebastion Lelong, Copyright © 2011..2021, All rights reserved.
Adapted-by | Rob Hamerling, Rob Jansen, Oliver "Kiste" Seitz
Compiler | 2.5r4

Description

    This library supports Peripheral Pin Select of 3 major groups
    of PICs, with significant differences in the PPS implementation:
       - 18F PICs with PPS (18FXXJ11, 18FXXJ13, 18FXXJ50, 18FXXJ53)
       - 18F PICs with PPS-light (high end PICs 18fxxj94/99)
       - Enhanced Midrange (16f15xx, 16f16xx, 16f17xx, 16f18xxx and lf variants).
    Within these groups there are minor differences, such that we distinguish
    5 PPS_GROUPS: PPS_1 for 18FxxJ11, 18FxxJ50
                  PPS_2 for 18FxxJ13, 18FxxJ53
                  PPS_3 for 18FxxJ94, 18FxxJ99
                  PPS_4 for 16F16xx, 16f17xx (without PMD0 register)
                  PPS_5 for 16F15xxx, 16f18xxx, 18FxxK40 (with PMD0 register)
    The actual PPS-group is specified in the device file of each PIC
     (PPS_0 when the PIC has no PPS).
    For all groups the basic rules with PPS are:
       * With OUTPUT a pin is assigned to a peripheral function
       * with INPUT the peripheral function is assigned to a pin.
    .
    Using PPS to (re-)configure a PIC involves 3 stages:
    1. The PPS module must be unlocked with:
          pps_control_lock(FALSE)
    2. Assign peripheral functions to specific pins.
       This stage is somewhat different for each of the major groups.
       PPS_1 and PPS_2:
          Example to (re)map pins TX2 and RX2 of the USART2 of a 18f27j53:
          To assign physical pin_B6 (alias pin_RP9) to the OUTPUT
          of the USART2 (TX2) specify:
                PPS_MAP_RP9 = PPS_TX2
          To assign INPUT of the USART2 (RX2) to physical pin_B7
          (alias RP10) specify:
                PPS_MAP_RX2 = RP10
       PPS_3:
          Not supported yet.
       PPS_4 and PPS_5:
          Example to (re)map pins TX and RX of the USART of a 16f1708:
          To assign physical pin_B7 to the OUTPUT of the USART (TX) specify:
                RC7PPS = PPS_TX
          To assign INPUT of the USART (RX) to physical pin_B6 specify:
                RXPPS = PPS_RB6
       For all PPS groups holds:
         -  Multiple peripheral functions can be mapped while the
            PPS module is unlocked.
         -  For bi-directional peripherals INPUT and OUTPUT must be
            mapped to the same physical pin.
    3. Finally the PPS module must be locked with:
          pps_control_lock(TRUE).
    .
    When 1-way locking is used with:
      - for groups PPS_1, 2 and 3:   pragma fuse_def IOL1WAY ENABLED
      - for groups 4 and 5:          pragma fuse_def PPS1WAY ENABLED
    peripheral pins can be assigned only once. When the PPS module is locked
    again further changes are ignored (until reset or power-off).
    This is the default behaviour of the PIC!
    When more than one unlock/remap/lock sequence is required specify:
      for groups PPS_1, 2 and 3:  pragma fuse_def IOL1WAY DISABLED
      for groups PPS_4 and 5:     pragma fuse_def PPS1WAY DISABLED

Sources

    Microchip TB3130 - Peripheral Pin Select in 8-Bit Microcontrollers Technical Brief
                       TB3098 - PIC16F170X Peripheral Pin Select (PPS) Technical Brief
                       Datasheets of the applicable PICs

Notes

    - This library is the original PPS library by Sebastien Lelong for
             the 18Fs, extended by Rob Hamerling for the Enhanced Midrange.

Dependencies

No dependency found

## Summary

### Global variables/contants

- `var bit pps_gie_state = 0`

### Procedures

- `pps_control_lock(bit in state)`

### Functions

## API details

### Global variables/contants

- `var bit pps_gie_state = 0`

### Procedures

- `pps_control_lock(bit in state)`

      Title:  Unlock/Lock the PPS module.
      Input:  Desired PPS lock state (bit: TRUE == locked, FALSE == unlocked)
      Returns: (nothing)
      Notes:  - Applies to all PPS-groups, differences are taken care of.
       Interrupts are disabled during the unlocked state.

### Functions

## Related samples

Here are the list of samples which use this library:

16f13115 | 16f13115_vl53l0x_continuous.jal
16f15324 | 16f15324_pwm3_pwm4_led.jal
16f15325 | 16f15325_adc.jal
16f15325 | 16f15325_stopwatch2.jal
16f15325 | 16f15325_stopwatch.jal
16f1579 | 16f1579_pwm1_16_bit_led.jal
16f1579 | 16f1579_pwm2_16_bit_led.jal
16f1579 | 16f1579_pwm4_16_bit_led.jal
16f1579 | 16f1579_pwm3_16_bit_led.jal
16f1708 | 16f1708_pps_serial_hw_int_cts.jal
16f1777 | 16f1777_pwm10_led.jal
16f1778 | 16f1778_pwm9_led.jal
16f1778 | 16f1778_pwm6_16_bit_led.jal
16f1778 | 16f1778_pwm3_led.jal
16f1778 | 16f1778_pwm4_led.jal
16f1778 | 16f1778_pwm5_16_bit_led.jal
16f1778 | 16f1778_pwm11_16_bit_led.jal
16f1779 | 16f1779_pwm12_16_bit_led.jal
16f18323 | 16f18323_adc.jal
16f18323 | 16f18323_pwm5_led.jal
16f18323 | 16f18323_pwm6_led.jal
16f18325 | 16f18325_i2c_hw_l0.jal
16f18325 | 16f18325_i2c_hw2_l0.jal
16f18425 | 16f18425_i2c_hw_l0.jal
16f18425 | 16f18425_i2c_hw2_l0.jal
16f18855 | 16f18855_pps_serial_hw_int_cts.jal
16f18857 | 16f18857_glcd_sh1106_font.jal
16f18857 | 16f18857_touch_interrupt_ads7843.jal
16f18857 | 16f18857_si5351a.jal
16f18857 | 16f18857_nec_rc_decoder_serial.jal
16f18857 | 16f18857_glcd_ssd1306_font.jal
16f18857 | 16f18857_glcd_ili9341_fat32_sd_card.jal
16f18857 | 16f18857_philips_rc_decoder_serial.jal
16f18857 | 16f18857_glcd_sh1106_font_graphics.jal
16f18857 | 16f18857_glcd_ssd1306_font_graphics.jal
16f18857 | 16f18857_glcd_ili9341.jal
16f18857 | 16f18857_touch_ads7843.jal
16f18857 | 16f18857_adc.jal
16f19176 | 16f19176_serial_hardware.jal
16f19176 | 16f19176_serial_hw2_int_cts.jal
16f19176 | 16f19176_serial_hardware2.jal
16f19176 | 16f19176_serial_hw_int_cts.jal
18f15q40 | 18f15q40_dma_usart.jal
18f15q40 | 18f15q40_spi2.jal
18f15q40 | 18f15q40_stopwatch2.jal
18f15q40 | 18f15q40_spi.jal
18f15q40 | 18f15q40_mcp23s08.jal
18f15q40 | 18f15q40_stopwatch.jal
18f15q40 | 18f15q40_memory_pointer.jal
18f15q40 | 18f15q40_dma_glcd_ili9341.jal
18f16q20 | 18f16q20_serial_hardware.jal
18f16q40 | 18f16q40_serial_hardware3.jal
18f16q40 | 18f16q40_serial_hw3_int_cts.jal
18f26j50 | 18f26j50_sd_card.jal
18f26j50 | 18f26j50_pps_rx2tx2.jal
18f26j50 | 18f26j50_fat32_sd_card.jal
18f26k42 | 18f26k42_serial_hardware.jal
18f26k42 | 18f26k42_serial_hardware2.jal
18f26k42 | 18f26k42_pwm6_led.jal
18f26k42 | 18f26k42_pwm7_led.jal
18f26k42 | 18f26k42_serial_hw_int_cts.jal
18f26k42 | 18f26k42_pwm5_led.jal
18f26k42 | 18f26k42_pwm8_led.jal
18f26k42 | 18f26k42_serial_hw2_int_cts.jal
18f27j53 | 18f27j53_pps_rx2tx2.jal
18f27j53 | 18f27j53_xbee_api_rx.jal
18f27j53 | 18f27j53_sd_card_minix_demo.jal
18f27j53 | 18f27j53_sd_card_minix_readi.jal
18f27j53 | 18f27j53_sd_card_minix_read.jal
18f46q10 | 18f46q10_glcd_ili9341_font.jal
18f47q43 | 18f47q43_serial_hardware2.jal
18f47q43 | 18f47q43_serial_hardware.jal
18f47q43 | 18f47q43_serial_hw_int_cts.jal
18f47q43 | 18f47q43_serial_hw3_int_cts.jal
18f47q43 | 18f47q43_serial_hw2_int_cts.jal
18f47q43 | 18f47q43_serial_hardware3.jal